**ANNEX II OF TENDER DOCUMENTATION TECHNICAL SPECIFICATIONS/**

**PRILOG II DOKUMENTACIJE ZA NADMETANJE TEHNIČKE SPECIFIKACIJE**

Subject of procurement is supply of the **EQUIPMENT FOR CLEANING OF CYLINDERS./**

Predmet nabave je nabava **OPREME ZA PRANJE VALJAKA.**

NOTE/NAPOMENA :

Tenderer shall complete column „Specifications offered“, defining in detail technical specifications of offered supplies (note: tenderer fills the exact specifications of offered supplies, the words “compliant” and , “equivalent „or “yes” etc. are not sufficient). Tenderer shall complete column „ Notes, remarks, references to documentation„ if it considers it necessary. Column „YES/NO“ is completed by the Contracting Authority. If not specified differently, Specifications Required are set out minimum technical requirements for the offered supplies and are not to be changed from the tenderer./

Ponuditelj obavezno popunjava stupac «Ponuđene karakteristike» definirajući detaljno tehničke specifikacije ponuđene robe (napomena: ponuditelj popunjava tehničke specifikacije upisujući točne karakteristike ponuđene robe, izbjegavajući pri tome popunjavanje stupca samo riječima kao što su npr. „zadovoljava“, „DA“, „jednakovrijedno traženom“ ili „odgovara traženom“). Stupac « Bilješke, napomene, reference na dokumentaciju » ponuditelj može popuniti ukoliko smatra potrebnim. Stupac « Ocjena DA/NE » ponuditelj ne popunjava s obzirom na to da je stupac predviđen za ocjene Naručitelja. Zahtjevi definirani Tehničkim specifikacijama predstavljaju minimalne tehničke karakteristike koje ponuđena roba mora zadovoljavati, ukoliko nije drugačije navedeno, te se iste ne smiju mijenjati od strane ponuditelja.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 1. Item/Stavka | | 2. Specifications Required/Tražene karakteristike | 3. Specifications  Offered/ Ponuđene  karakteristike | 4. Notes, remarks, references to documentation/ Bilješke, napomene, reference na dokumentaciju | 5. Notes (yes/no)/  Ocjene (da/ne) |
| 1. | High-Pressure Washing Machine/Perilica valjaka | Automatic washing machine for washing (cleaning) all types anilox rollers, sleeves and gravure cylinders.  max. length for rollers and cylinders: 2000 mm  max. length for sleeves: 1700 mm  max. diameter (sleeves, rollers, cylinders): 250 mm  max. weight (sleeves, rollers, cylinders): 380 kg/  Automatska perilica za pranje/čišćenje svih vrsta raster valjaka, košuljica i graviranih cilindara.  Maksimalna duljina valjaka i cilindara: 2000 mm  Maksimalna duljina košuljica: 1700 mm  Maksimalni promjer: 250 m  Maksimalna težina: 380 kg |  |  |  |
| 2. | Option/Opcija | Support disks Anilox Rollers/  Diskovi za pridržavanje Anilox valjaka |  |  |  |
| 3. | Documentation/Dokumentacija | -Operating instructions/Radne upute  -Technical manual/Tehnička uputstva  -Spare part list/Lista rezervnih djelova |  |  |  |
| 4. | Other/Ostalo | -Installation/Ugradnja  -Commissioning/Puštanje u rad |  |  |  |
| 5. | Warranty/Jamstvo | A warranty period of at least two years/  Jamstveni period od minimalno dvije godine |  |  |  |