**ANNEX II OF TENDER DOCUMENTATION TECHNICAL SPECIFICATIONS/**

**PRILOG II DOKUMENTACIJE ZA NADMETANJE TEHNIČKE SPECIFIKACIJE**

Subject of procurement is supply and delivery of solvent DBE

Predmet nabave je nabava i dostava otapala DBE

Dibasic ester/Dibasic ester

NOTE/NAPOMENA :

Tenderer shall complete column „Specifications offered“, defining in detail technical specifications of offered supplies (note: tenderer fills the exact specifications of offered supplies, the words “compliant” and , “equivalent „or “yes” etc. are not sufficient). Tenderer shall complete column „ Notes, remarks, references to documentation„ if it considers it necessary. Column „YES/NO“ is completed by the Contracting Authority. If not specified differently, Specifications Required are set out minimum technical requirements for the offered supplies and are not to be changed from the tenderer./

Ponuditelj obavezno popunjava stupac «Ponuđene karakteristike» definirajući detaljno tehničke specifikacije ponuđene robe (napomena: ponuditelj popunjava tehničke specifikacije upisujući točne karakteristike ponuđene robe, izbjegavajući pri tome popunjavanje stupca samo riječima kao što su npr. „zadovoljava“, „DA“, „jednakovrijedno traženom“ ili „odgovara traženom“). Stupac « Bilješke, napomene, reference na dokumentaciju » ponuditelj može popuniti ukoliko smatra potrebnim. Stupac « Ocjena DA/NE » ponuditelj ne popunjava s obzirom na to da je stupac predviđen za ocjene Naručitelja. Zahtjevi definirani Tehničkim specifikacijama predstavljaju minimalne tehničke karakteristike koje ponuđena roba mora zadovoljavati, ukoliko nije drugačije navedeno, te se iste ne smiju mijenjati od strane ponuditelja.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1. Item/Stavka** | **2. Specifications Required/Tražene karakteristike** | **3. Specifications** **Offered/ Ponuđene** **karakteristike** | **4. Notes, remarks, references to documentation/ Bilješke, napomene, reference na dokumentaciju** | **5. Notes (yes/no)/** **Ocjene (da/ne)** |
| **1.** | **Purpose/Namjena** | Solvent/Otapalo |  |  |  |
| **2.**  | **Ester content/Sadržaj estera** | 99,0% min (Method GC or equivalent / Metoda GC ili jednakovrijedno) |  |  |  |
| **2.1** | **Dimethylsuccinate** | 15-25% (Method or equivalent / Metoda GC ili jednakovrijedno) |  |  |  |
| **2.2** | **Dimethylglutarate** | 55-65% (Method GC or equivalent / Metoda GC ili jednakovrijedno) |  |  |  |
| **2.3** | **Dimethyladipate** | 10-25% (Method GC or equivalent / Metoda GC ili jednakovrijedno) |  |  |  |
| **3.** | **Density/Gustoća**  | 1,080 – 1,096g/cm3 (DIN 51757 or equivalent/ ili jednakovrijedno) |  |  |  |
| **4.** | **Water/Voda** | 0,1% max (DIN 51777 or equivalent/ ili jednakovrijedno) |  |  |  |
| **5.** | **Colour/Boja** | 15 Max. Pt-Co (DIN ISO 6271 or equivalent/ ili jednakovrijedno) |  |  |  |
| **6.** | **Dokumentacija/Dokumentation:** | - Statement of conformity/ Certifikat o sukladnosti- Allergen statement/ Izjava o alergenima-Supplier technical data sheet/ Tehnički list dobavljača |  |  |  |